|  |  |
| --- | --- |
| 3GPP TS 38.101-1 V18.8.0 (2024-12) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  NR;  User Equipment (UE) radio transmission and reception;  Part 1: Range 1 Standalone  (Release 18) | |
|  | |
|  |  |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 24

1 Scope 26

2 References 26

3 Definitions, symbols and abbreviations 27

3.1 Definitions 27

3.2 Symbols 28

3.3 Abbreviations 31

4 General 32

4.1 Relationship between minimum requirements and test requirements 32

4.2 Applicability of minimum requirements 32

4.3 Specification suffix information 33

5 Operating bands and channel arrangement 34

5.1 General 34

5.2 Operating bands 34

5.2A Operating bands for CA 36

5.2A.0 General 36

5.2A.1 Intra-band CA 36

5.2A.2 Inter-band CA 37

5.2A.2.1 Inter-band CA (two bands) 38

5.2A.2.2 Inter-band CA (three bands) 42

5.2A.2.3 Inter-band CA (four bands) 48

5.2A.2.4 Inter-band CA (five bands) 51

5.2A.2.5 Inter-band CA (six bands) 51

5.2B Operating bands for DC 51

5.2C Operating band combination for SUL 52

5.2D Operating bands for UL MIMO 54

5.2E Operating band for V2X 55

5.2E.1 V2X operating bands 55

5.2E.1A Sidelink CA operating bands 55

5.2E.1F Operating bands for Sidelink Unlicensed 55

5.2E.2 V2X operating bands for concurrent operation 56

5.2E.2F Operating bands for SL-U concurrent operation 56

5.2J Operating band for ATG 56

5.2K Operating bands for Aerial UE 57

5.3 UE channel bandwidth 57

5.3.1 General 57

5.3.2 Maximum transmission bandwidth configuration 58

5.3.3 Minimum guardband and transmission bandwidth configuration 58

5.3.4 RB alignment 60

5.3.5 UE channel bandwidth per operating band 60

5.3.6 Asymmetric channel bandwidths 67

5.3A UE channel bandwidth for CA 68

5.3A.1 General 68

5.3A.2 Maximum transmission bandwidth configuration for CA 68

5.3A.3 Minimum guardband and transmission bandwidth configuration for CA 68

5.3A.4 Void 70

5.3A.5 UE channel bandwidth per operating band for CA 70

5.3E Channel bandwidth for V2X 71

5.3E.1 General 71

5.3E.1A Channel bandwidth for Sidelink CA 71

5.3E.1F Channel bandwidth for Sidelink Unlicensed 72

5.3E.2 Channel bandwidth for V2X concurrent operation 73

5.3E.2F Channel bandwidth for SL-U concurrent operation 74

5.3I Channel bandwidth for (e)RedCap 75

5.4 Channel arrangement 75

5.4.1 Channel spacing 75

5.4.1.1 Channel spacing for adjacent NR carriers 75

5.4.2 Channel raster 75

5.4.2.1 NR-ARFCN and channel raster 75

5.4.2.2 Channel raster to resource element mapping 76

5.4.2.3 Channel raster entries for each operating band 76

5.4.3 Synchronization raster 80

5.4.3.1 Synchronization raster and numbering 80

5.4.3.3 Synchronization raster entries for each operating band 81

5.4.4 TX–RX frequency separation 83

5.4A Channel arrangement for CA 84

5.4A.1 Channel spacing for CA 84

5.4A.2 Channel raster for CA 85

5.4A.3 Synchronization raster for CA 85

5.4A.4 Tx-Rx frequency separation for CA 85

5.4B Reserved 85

5.4C Reserved 85

5.4D Reserved 85

5.4E Channel arrangement for V2X 85

5.4E.1 Channel spacing 85

5.4E.1A Channel spacing for Sidelink CA 85

5.4E.1F Channel spacing for Sidelink Unlicensed 86

5.4E.2 Channel raster 86

5.4E.2.1 NR-ARFCN and channel raster 86

5.4E.2.1A Void 86

5.4E.2.1F Void 86

5.4E.2.2 Channel raster to resource element mapping 86

5.4E.2.2A Void 86

5.4E.2.2F Void 86

5.4E.2.3 Channel raster entries for each operating band 86

5.4E.2.3A Void 86

5.4E.2.3F Void 86

5.4E.3 Synchronization raster for V2X 87

5.4E.3A Synchronization raster for Sidelink CA 87

5.4E.3F Synchronization raster for Sidelink Unlicensed 87

5.4I Channel arrangement for (e)RedCap 87

5.4I.1 Channel spacing for (e)RedCap 87

5.4I.2 Channel raster for (e)RedCap 88

5.4I.2.1 NR-ARFCN and channel raster 88

5.4I.2.2 Channel raster to resource element mapping 88

5.4I.2.3 Channel raster entries for each operating band 88

5.4I.3 Synchronization raster for (e)RedCap 88

5.4I.4 Tx-Rx frequency separation for (e)RedCap 88

5.5 Void 89

5.5A Configurations for CA 89

5.5A.0 General 89

5.5A.1 Configurations for intra-band contiguous CA 90

5.5A.2 Configurations for intra-band non-contiguous CA 93

5.5A.3 Configurations for inter-band CA 98

5.5A.3.0 General 98

5.5A.3.1 Configurations for inter-band CA (two bands) 98

Table 5.5A.3.1-1a ~ Table 5.5A.3.1-1e 98

Table 5.5A.3.1-1f ~ Table 5.5A.3.1-1j 115

Table 5.5A.3.1-1k ~ Table 5.5A.3.1-1n 133

5.5A.3.2 Configurations for inter-band CA (three bands) 148

Table 5.5A.3.2-1a 148

Table 5.5A.3.2-1b 209

Table 5.5A.3.2-1c 259

5.5A.3.3 Configurations for inter-band CA (four bands) 281

Table 5.5A.3.3-1a 282

Table 5.5A.3.3-1b 334

5.5A.3.4 Configurations for inter-band CA (five bands) 380

5.5A.3.5 Configurations for inter-band CA (six bands) 403

5.5B Configurations for DC 405

5.5C Configurations for SUL 419

5.5D Reserved 430

5.5E Void 430

5.5E.1A Configurations for Sidelink CA 430

5.5E.1A.1 Configurations for Sidelink intra-band contiguous CA 430

6 Transmitter characteristics 431

6.1 General 431

6.1A General 431

6.1F General 431

6.1G (Reserved) 431

6.1H (Reserved) 431

6.1I (Reserved) 431

6.1J General 431

6.1K (Reserved) 432

6.1L (Reserved) 432

6.2 Transmitter power 432

6.2.1 UE maximum output power 432

6.2.1I Void 434

6.2.2 UE maximum output power reduction 434

6.2.3 UE additional maximum output power reduction 437

6.2.3.1 General 437

6.2.3.2 A-MPR for NS\_04 441

6.2.3.3 A-MPR for NS\_10 445

6.2.3.4 A-MPR for NS\_05 and NS\_05U 446

6.2.3.5 A-MPR for NS\_40 449

6.2.3.6 A-MPR for NS\_43 and NS\_43U 450

6.2.3.7 A-MPR for NS\_03 and NS\_03U 452

6.2.3.8 A-MPR for NS\_37 453

6.2.3.9 A-MPR for NS\_38 454

6.2.3.10 A-MPR for NS\_39 454

6.2.3.11 A-MPR for NS\_41 455

6.2.3.12 A-MPR for NS\_42 455

6.2.3.13 A-MPR for NS\_18 456

6.2.3.14 A-MPR for NS\_21 457

6.2.3.15 A-MPR for NS\_24 459

6.2.3.16 A-MPR for NS\_27 460

6.2.3.17 A-MPR for NS\_46 462

6.2.3.18 A-MPR for NS\_47 466

6.2.3.19 A-MPR for NS\_50 468

6.2.3.20 A-MPR for NS\_44 471

6.2.3.21 A-MPR for NS\_12 472

6.2.3.22 A-MPR for NS\_13 472

6.2.3.23 A-MPR for NS\_14 473

6.2.3.24 A-MPR for NS\_15 473

6.2.3.25 A-MPR for NS\_45 474

6.2.3.26 A-MPR for NS\_48 475

6.2.3.27 A-MPR for NS\_49 477

6.2.3.28 A-MPR for NS\_51 479

6.2.3.29 A-MPR for NS\_07 480

6.2.3.30 A-MPR for NS\_56 481

6.2.3.31 A-MPR for NS\_35 482

6.2.3.32 A-MPR for NS\_06 482

6.2.4 Configured transmitted power 483

6.2A Transmitter power for CA 488

6.2A.0 General 488

6.2A.1 UE maximum output power for CA 488

6.2A.1.1 UE maximum output power for Intra-band contiguous CA 488

6.2A.1.2 UE maximum output power for Intra-band non-contiguous CA 489

6.2A.1.3 UE maximum output power for Inter-band CA 489

6.2A.1.4 Void 495

6.2A.1.5 Void 495

6.2A.2 UE maximum output power reduction for CA 495

6.2A.2.1 UE maximum output power reduction for Intra-band contiguous CA 495

6.2A.2.2 UE maximum output power reduction for Intra-band non-contiguous CA 498

6.2A.2.2.0 General 498

6.2A.2.2.1 MPR to meet -30dBm/MHz 500

6.2A.2.2.1.1 PC3 with indicating dualPA-Architecture supported 500

6.2A.2.2.1.2 PC2 with indicating dualPA-Architecture supported 500

6.2A.2.2.1.3 PC3 without indicating dualPA-Architecture supported 500

6.2A.2.2.1.4 PC2 without indicating dualPA-Architecture supported 501

6.2A.2.2.2 MPR to meet -13dBm/MHz 501

6.2A.2.2.2.1 PC3 with indicating dualPA-Architecture supported 501

6.2A.2.2.2.2 PC2 with indicating dualPA-Architecture supported 502

6.2A.2.2.2.3 PC3 without indicating dualPA-Architecture supported 502

6.2A.2.2.2.4 PC2 without indicating dualPA-Architecture supported 502

6.2A.2.3 UE maximum output power reduction for Inter-band CA 503

6.2A.2.4 Void 503

6.2A.3 UE additional maximum output power reduction for CA 503

6.2A.3.1 UE additional maximum output power reduction for Intra-band CA 503

6.2A.3.1.1 UE additional maximum output power reduction for Intra-band contiguous CA 503

6.2A.3.1.1.1 A-MPR for CA\_NS\_04 504

6.2A.3.1.1.1.1 Contiguous allocations 504

6.2A.3.1.1.1.2 Non-contiguous allocations 505

6.2A.3.1.2 UE additional maximum output power reduction for Intra-band non-contiguous CA 511

6.2A.3.1.3 UE additional maximum output power reduction for Inter-band CA 514

6.2A.4 Configured output power for CA 516

6.2A.4.1 Configured transmitted power level 516

6.2A.4.1.1 Configured transmitted power for Intra-band contiguous CA 516

6.2A.4.1.2 Configured transmitted power for Intra-band non-contiguous CA 519

6.2A.4.1.3 Configured transmitted power for Inter-band CA 522

6.2A.4.1.4 Void 526

6.2A.4.2 ΔTIB,c for CA 526

6.2A.4.2.1 Void 526

6.2A.4.2.2 Void 526

6.2A.4.2.3 ΔTIB,c for Inter-band CA (two bands) 526

6.2A.4.2.4 ΔTIB,c for Inter-band CA (three bands) 530

6.2A.4.2.5 ΔTIB,c for Inter-band CA (four bands) 537

6.2A.4.2.6 ΔTIB,c for Inter-band CA (five bands) 540

6.2A.4.2.7 ΔTIB,c for Inter-band CA (six bands) 540

6.2B Transmitter power for NR-DC 541

6.2B.0 General 541

6.2B.1 UE maximum output power for NR-DC 541

6.2B.2 UE maximum output power reduction for NR-DC 542

6.2B.3 UE additional maximum output power reduction for NR-DC 543

6.2B.4.1 Configured transmitted power level for NR-DC 543

6.2B.4.2 ΔTIB,c for NR-DC 547

6.2C Transmitter power for SUL 547

6.2C.1 Configured transmitted power for SUL 547

6.2C.2 ΔTIB,c 548

6.2D Transmitter power for UL MIMO 551

6.2D.1 UE maximum output power for UL MIMO 551

6.2D.2 UE maximum output power reduction for UL MIMO 553

6.2D.3 UE additional maximum output power reduction for UL MIMO 556

6.2D.4 Configured transmitted power for UL MIMO 556

6.2E Transmitter power for V2X 557

6.2E.1 UE maximum output power for V2X 557

6.2E.1.1 General 557

6.2E.1.1A Void 558

6.2E.1.2 UE maximum output power for V2X concurrent operation 558

6.2E.1A UE maximum output power for Sidelink CA 560

6.2E.1F UE maximum output power for Sidelink Unlicensed 560

6.2E.1F.1 General 560

6.2E.1.2F Void 561

6.2E.1F.2 UE Maximum output power for SL-U concurrent operation 561

6.2E.2 UE maximum output power reduction for V2X 562

6.2E.2.1 General 562

6.2E.2.1A MPR for sidelink CA 562

6.2E.2.2 MPR for Power class 2 and Power class 3 V2X UE 563

6.2E.2.3 MPR for Power class 2 and Power class 3 V2X concurrent operation 565

6.2E.2.4 MPR for Power class 1 UE in Band n14 568

6.2E.2F UE maximum output power reduction for Sidelink Unlicensed 568

6.2E.2F.1 General 568

6.2E.2F.2 MPR for NR SL-U UE 568

6.2E.2F.3 MPR for SL-U concurrent operation 570

6.2E.3 UE additional maximum output power reduction for V2X 570

6.2E.3.1 General 570

6.2E.3.2 A-MPR for V2X UE by NS\_33 571

6.2E.3.3 A-MPR for Power class 3 V2X UE by NS\_52 575

6.2E.3.4 A-MPR for V2X concurrent operation 576

6.2E.3F UE additional maximum output power reduction for Sidelink Unlicensed 577

6.2E.3F.1 General 577

6.2E.3F.2 A-MPR for NS\_31 578

6.2E.3F.3 Void 579

6.2E.3F.4 Void 579

6.2E.3F.5 Void 579

6.2E.3F.6 A-MPR for NS\_61 579

6.2E.3F.7 A-MPR for SL-U concurrent operation 580

6.2E.3F.8 A-MPR for NS\_28 580

6.2E.3F.9 A-MPR for NS\_29 582

6.2E.3F.10 A-MPR for NS\_30 583

6.2E.3F.11 A-MPR for NS\_54 585

6.2E.3F.12 A-MPR for NS\_64 586

6.2E.3F.13 A-MPR for NS\_65 588

6.2E.3F.14 A-MPR for NS\_66 589

6.2E.3F.15 A-MPR for NS\_67 or NS\_71 590

6.2E.3F.16 A-MPR for NS\_68 591

6.2E.3F.17 A-MPR for NS\_69 592

6.2E.4 Configured transmitted power for V2X 593

6.2E.4.1 General 593

6.2E.4.2 Configured transmitted power for inter-band V2X concurrent operation 594

6.2E.4.3 Configured transmitted power for intra-band V2X concurrent operation 595

6.2E.4A Configured transmitted power for Sidelink CA 597

6.2E.4F Configured transmitted power for Sidelink Unlicensed 598

6.2E.4F.1 General 598

6.2E.4F.2 Configured transmitted power for inter-band concurrent operation 599

6.2F Transmitter power for shared spectrum channel access 600

6.2F.1 UE maximum output power 600

6.2F.1A UE maximum output power for CA 601

6.2F.1A.1 UE maximum output power for inter-band CA 601

6.2F.1A.2 UE maximum output power for intra-band contiguous CA 602

6.2F.1A.2.1 Additional requirements for transmit power density for intra-band contiguous CA for CA\_NS\_53 602

6.2F.1A.2.2 Additional requirements for transmit power density for intra-band contiguous CA for CA\_NS\_54 602

6.2F.1B UE maximum output power for NR-DC 603

6.2F.1D UE maximum output power for UL MIMO 603

6.2F.2 UE maximum output power reduction 603

6.2F.2A UE maximum output power reduction for CA 606

6.2F.2A.1 UE maximum output power reduction for inter-band CA 606

6.2F.2A.2 UE maximum output power reduction for intra-band contiguous CA 606

6.2F.2D UE maximum output power reduction for UL MIMO 609

6.2F.3 UE additional maximum output power reduction 609

6.2F.3.1 General 609

6.2F.3.2 A-MPR for NS\_28 610

6.2F.3.3 A-MPR for NS\_29 611

6.2F.3.4 A-MPR for NS\_30 612

6.2F.3.5 A-MPR for NS\_31 613

6.2F.3.6 A-MPR for NS\_53 614

6.2F.3.7 A-MPR for NS\_54 614

6.2F.3.8 A-MPR for NS\_58 615

6.2F.3.9 A-MPR for NS\_59 616

6.2F.3.10 A-MPR for NS\_60 617

6.2F.3.11 A-MPR for NS\_61 618

6.2F.3.12 A-MPR for NS\_63 619

6.2F.3.13 A-MPR for NS\_64 620

6.2F.3.14 A-MPR for NS\_65 620

6.2F.3.15 A-MPR for NS\_66 621

6.2F.3.16 A-MPR for "NS\_67" or "NS\_71" 621

6.2F.3.17 A-MPR for NS\_68 622

6.2F.3.18 A-MPR for NS\_69 622

6.2F.3A UE additional maximum output power reduction for CA 623

6.2F.3A.1 UE additional maximum output power reduction for inter-band CA 623

6.2F.3A.2 UE additional maximum output power reduction for intra-band CA 623

6.2F.3A.2.0 General 623

6.2F.3A.2.1 UE additional maximum output power reduction for intra-band contiguous CA 623

6.2F.3A.2.2 A-MPR for CA\_NS\_53 625

6.2F.3A.2.3 A-MPR for CA\_NS\_54 626

6.2F.3D UE additional maximum output power reduction for UL MIMO 626

6.2F.4 Configured transmitted power 626

6.2F.4D Configured transmitted power UL MIMO 626

6.2G Transmitter power for Tx Diversity 627

6.2G.1 UE maximum output power for Tx Diversity 627

6.2G.2 UE maximum output power reduction for Tx Diversity 627

6.2G.3 UE additional maximum output power reduction for Tx Diversity 627

6.2G.4 Configured transmitted power for Tx Diversity 627

6.2H Transmitter power for CA with UL MIMO 628

6.2H.1 Transmitter power for intra-band UL contiguous CA with UL MIMO 628

6.2H.1.1 UE maximum output power for intra-band UL contiguous CA with UL MIMO 628

6.2H.1.2 UE maximum output power reduction for intra-band UL contiguous CA with UL MIMO 629

6.2H.1.3 UE additional maximum output power reduction for intra-band UL contiguous CA with UL MIMO 629

6.2H.1.4 Configured transmitted power for intra-band UL contiguous CA with UL MIMO 629

6.2H.2 Void 630

6.2H.3 Transmitter power for inter-band UL CA with UL MIMO 630

6.2H.3.1 UE maximum output power for inter-band UL CA with UL MIMO 630

6.2H.3.2 UE maximum output power reduction for inter-band UL CA with UL MIMO 632

6.2H.3.3 UE additional maximum output power reduction for inter-band UL CA with UL MIMO 632

6.2H.3.4 Configured transmitted power for inter-band UL CA with UL MIMO 632

6.2I Transmitter power for (e)RedCap 632

6.2I.1 Maximum output power for RedCap 632

6.2J Transmitter power for ATG 633

6.2J.1 UE maximum output power for ATG 633

6.2J.2 Configured transmitted power for ATG 633

6.2K Transmitter power for Aerial UE 634

6.2K.1 Maximum output power for Aerial UE 634

6.2K.2 Maximum output power reduction for Aerial UE 634

6.2K.3 Additional maximum output power reduction for Aerial UE 634

6.2K.3.1 General 634

6.2K.3.2 A-MPR for NS\_UAV\_44 635

6.2K.3.3 A-MPR for NS\_UAV\_70 636

6.2K.4 Configured transmitted power for Aerial UE 637

6.2L Transmitter power for CA with Tx Diversity 637

6.2L.1 Void 637

6.2L.2 Void 637

6.2L.3 Transmitter power for inter-band UL CA with Tx Diversity 637

6.2L.3.1 UE maximum output power for inter-band UL CA with Tx Diversity 637

6.2L.3.2 UE maximum output power reduction for inter-band UL CA with Tx Diversity 639

6.2L.3.3 UE additional maximum output power reduction for inter-band UL CA with Tx Diversity 639

6.2L.3.4 Configured transmitted power for inter-band UL CA with Tx Diversity 640

6.3 Output power dynamics 640

6.3.1 Minimum output power 640

6.3.2 Transmit OFF power 640

6.3.3 Transmit ON/OFF time mask 641

6.3.3.1 General 641

6.3.3.2 General ON/OFF time mask 641

6.3.3.3 Transmit power time mask for slot and short or long subslot boundaries 641

6.3.3.4 PRACH time mask 642

6.3.3.5 Void 643

6.3.3.6 SRS time mask 643

6.3.3.7 PUSCH-PUCCH and PUSCH-SRS time masks 644

6.3.3.8 Transmit power time mask for consecutive slot or long subslot transmission and short subslot transmission boundaries 645

6.3.3.9 Transmit power time mask for consecutive short subslot transmissions boundaries 646

6.3.4 Power control 646

6.3.4.1 General 646

6.3.4.2 Absolute power tolerance 646

6.3.4.3 Relative power tolerance 647

6.3.4.4 Aggregate power tolerance 647

6.3A Output power dynamics for CA 648

6.3A.1 Minimum output power for CA 648

6.3A.1.1 Minimum output power for intra-band contiguous CA 648

6.3A.1.2 Minimum output power for intra-band non-contiguous CA 648

6.3A.1.3 Minimum output power for inter-band CA 648

6.3A.1.4 Void 648

6.3A.2 Transmit OFF power for CA 648

6.3A.2.1 Transmit OFF power for intra-band contiguous CA 648

6.3A.2.2 Transmit OFF power for intra-band non-contiguous CA 648

6.3A.2.3 Transmit OFF power for inter-band CA 648

6.3A.2.4 Void 649

6.3A.3 Transmit ON/OFF time mask for CA 649

6.3A.3.1 Transmit ON/OFF time mask for intra-band contiguous CA 649

6.3A.3.2 Transmit ON/OFF time mask for intra-band non-contiguous CA 649

6.3A.3.3 Transmit ON/OFF time mask for inter-band CA 649

6.3A.3.3.1 General 649

6.3A.3.3.2 Time mask for switching between two uplink carriers 650

6.3A.3.3.3 Time mask for switching between two uplink carriers with two transmit antenna connectors 651

6.3A.3.3.4 Time mask for switching between one uplink band with one transmit antenna connector and one uplink band with two transmit antenna connectors 652

6.3A.3.3.5 Time mask for switching between two uplink bands with two transmit antenna connectors 654

6.3A.3.3.6 Time mask for switching across up to four uplink bands 655

6.3A.3.3.6a Additional requirements for three-band switching with dual TAG 659

6.3A.3.4 Void 659

6.3A.4 Power control for CA 659

6.3A.4.1 Power control for intra-band contiguous CA 659

6.3A.4.1.1 Absolute power tolerance 659

6.3A.4.1.2 Relative power tolerance 659

6.3A.4.1.3 Aggregate power control tolerance 660

6.3A.4.2 Power control for intra-band non-contiguous CA 660

6.3A.4.2.1 Absolute power tolerance 660

6.3A.4.2.1.1 Minimum requirements 660

6.3A.4.2.2 Relative power tolerance 660

6.3A.4.2.2.1 Minimum requirements 660

6.3A.4.2.3 Aggregate power control tolerance 660

6.3A.4.3 Power control for inter-band CA 660

6.3A.4.4 Void 660

6.3B Output power dynamics for NR-DC 660

6.3C Output power dynamics for SUL 661

6.3C.1 Void 661

6.3C.2 Void 661

6.3C.3 Transmit ON/OFF time mask for SUL 661

6.3C.3.0 General 661

6.3C.3.1 Time mask for switching between two uplink carriers 661

6.3C.3.2 Time mask for switching between two uplink carriers with two transmit antenna connectors 662

6.3C.3.3 Time mask for switching between one uplink band with one transmit antenna connector and one uplink band with two transmit antenna connectors 663

6.3C.3.4 Time mask for switching between two uplink bands with two transmit antenna connectors 665

6.3C.3.5 Time mask for switching across up to four uplink bands 666

6.3C.3.5a Additional requirements for three-band switching with dual TAG 670

6.3D Output power dynamics for UL MIMO 670

6.3D.1 Minimum output power for UL MIMO 670

6.3D.2 Transmit OFF power for UL MIMO 670

6.3D.3 Transmit ON/OFF time mask for UL MIMO 670

6.3D.4 Power control for UL MIMO 670

6.3E Output power dynamics for V2X 671

6.3E.1 Minimum output power for V2X 671

6.3E.1.1 General 671

6.3E.1.1A Minimum output power for sidelink CA 671

6.3E.1.2 Minimum output power for V2X concurrent operation 671

6.3E.1F Minimum output power for Sidelink Unlicensed 671

6.3E.1F.1 Minimum output power for SL-U concurrent operation 672

6.3E.2 Transmit OFF power for V2X 672

6.3E.2.1 General 672

6.3E.2.1A Transmit OFF power for sidelink CA 672

6.3E.2.2 Transmit OFF power for V2X concurrent operation 672

6.3E.2F Transmit OFF power for Sidelink Unlicensed 672

6.3E.2F.1 Transmit OFF power for SL-U concurrent operation 673

6.3E.3 Transmit ON/OFF time mask for V2X 673

6.3E.3.1 General 673

6.3E.3.1A Transmit ON/OFF time mask for sidelink CA 673

6.3E.3.2 General time mask 673

6.3E.3.3 S-SSB time mask 673

6.3E.3.4 Transmit ON/OFF time mask for V2X concurrent operation 674

6.3E.3F Transmit ON/OFF time mask for Sidelink Unlicensed 675

6.3E.3F.1 General 675

6.3E.3F.2 General ON/OFF time mask 675

6.3E.3F.3 S-SSB time mask 676

6.3E.3F.4 Transmit ON/OFF time mask for NR SL-U concurrent operation 676

6.3E.4 Power control for V2X 676

6.3E.4.1 General 676

6.3E.4.1A Power control for sidelink CA 676

6.3E.4.2 Absolute power tolerance 676

6.3E.4.3 Power control for V2X concurrent operation 677

6.3E.4F Power control for Sidelink Unlicensed 677

6.3E.4F.1 General 677

6.3E.4F.2 Absolute power tolerance 677

6.3E.4F.3 Power control for SL-U concurrent operation 677

6.3F Output power dynamics for shared spectrum channel access 677

6.3F.1 Minimum output power 677

6.3F.2 Transmit OFF power 677

6.3F.3 Transmit ON/OFF time mask 677

6.3F.3.1 General 677

6.3F.3.2 General ON/OFF time mask 677

6.3F.3A General ON/OFF mask for CA 678

6.3F.3A.1 General ON/OFF mask for inter-band CA 678

6.3F.4 Power control 678

6.3F.4.1 General 678

6.3F.4.2 Absolute power tolerance 678

6.3F.4.3 Relative power tolerance 678

6.3F.4.4 Aggregate power tolerance 678

6.3F.4A Power control for inter-band CA 678

6.3G Output power dynamics for Tx Diversity 679

6.3G.1 Minimum output power for Tx Diversity 679

6.3G.2 Transmit OFF power for Tx Diversity 679

6.3G.3 Transmit ON/OFF time mask for Tx Diversity 679

6.3G.4 Power control for Tx Diversity 679

6.3H Output power dynamics for CA with UL MIMO 679

6.3H.1 Output power dynamics for intra-band UL contiguous CA with UL MIMO 679

6.3H.1.1 Minimum output power for intra-band UL contiguous CA with UL MIMO 679

6.3H.1.2 Transmit OFF power for intra-band UL contiguous CA with UL MIMO 679

6.3H.1.3 Transmit ON/OFF time mask for intra-band UL contiguous CA with UL MIMO 679

6.3H.1.4 Power control for intra-band UL contiguous CA with UL MIMO 680

6.3H.3 Output power dynamics for inter-band UL CA with UL MIMO 680

6.3H.3.1 Minimum output power for inter-band UL CA with UL MIMO 680

6.3H.3.2 Transmit OFF power for inter-band UL CA with UL MIMO 680

6.3H.3.3 Transmit ON/OFF time mask for inter-band UL CA with UL MIMO 680

6.3H.3.4 Power control for inter-band UL CA with UL MIMO 680

6.3I (Reserved) 680

6.3J Output power dynamics for ATG 680

6.3J.1 Minimum output power for ATG 680

6.3J.2 Transmit OFF power for ATG 681

6.3J.3 Transmit ON/OFF time mask for ATG 681

6.3J.4 Power control for ATG 681

6.3K (Reserved) 681

6.3L Output power dynamics for CA with Tx Diversity 681

6.3L.1 Void 681

6.3L.2 Void 681

6.3L.3 Output power dynamics for inter-band UL CA with Tx Diversity 681

6.3L.3.1 Minimum output power for inter-band UL CA with Tx Diversity 681

6.3L.3.2 Transmit OFF power for inter-band UL CA with Tx Diversity 682

6.3L.3.3 Transmit ON/OFF time mask for inter-band UL CA with Tx Diversity 682

6.3L.3.4 Power control for inter-band UL CA with Tx Diversity 682

6.4 Transmit signal quality 682

6.4.1 Frequency error 682

6.4.2 Transmit modulation quality 682

6.4.2.0 General 682

6.4.2.1 Error Vector Magnitude 682

6.4.2.1a Error Vector Magnitude including symbols with transient period 683

6.4.2.2 Carrier leakage 684

6.4.2.3 In-band emissions 684

6.4.2.4 EVM equalizer spectrum flatness 685

6.4.2.4.1 Requirements for Pi/2 BPSK modulation with *powerBoosting-pi2BPSK* capability 686

6.4.2.4.2 Requirements for Pi/2 BPSK and QPSK modulation with *powerBoosting-pi2BPSK-QPSK-Modified-r18* capability 687

6.4.2.5 Phase continuity requirements for DMRS bundling 688

6.4A Transmit signal quality for CA 689

6.4A.1 Frequency error for CA 689

6.4A.1.1 Frequency error for intra-band contiguous CA 689

6.4A.1.2 Frequency error for intra-band non-contiguous CA 689

6.4A.1.3 Frequency error for inter-band CA 689

6.4A.1.4 Void 690

6.4A.2 Transmit modulation quality for CA 690

6.4A.2.1 Transmit modulation quality for intra-band contiguous CA 690

6.4A.2.1.0 General 690

6.4A.2.1.1 Error Vector Magnitude 690

6.4A.2.1.2 In-band emissions 690

6.4A.2.1.3 Carrier leakage 693

6.4A.2.2 Transmit modulation quality for intra-band non-contiguous CA 693

6.4A.2.2.0 General 693

6.4A.2.2.1 Error Vector Magnitude 693

6.4A.2.2.2 In-band emissions 694

6.4A.2.2.3 Carrier leakage 694

6.4A.2.3 Transmit modulation quality for inter-band CA 694

6.4A.2.4 Void 695

6.4B Transmit signal quality for NR-DC 695

6.4C Transmit signal quality for SUL 695

6.4D Transmit signal quality for UL MIMO 695

6.4D.0 General 695

6.4D.1 Frequency error for UL MIMO 695

6.4D.2 Transmit modulation quality for UL MIMO 696

6.4D.2.0 General 696

6.4D.2.1 Error Vector Magnitude 696

6.4D.2.2 Carrier leakage 696

6.4D.2.3 In-band emissions 696

6.4D.2.4 EVM equalizer spectrum flatness for UL MIMO 696

6.4D.3 Time alignment error for UL MIMO 696

6.4D.4 Requirements for coherent UL MIMO 697

6.4E Transmit signal quality for V2X 697

6.4E.1 Frequency error for V2X 697

6.4E.1.1 General 697

6.4E.1.1A Frequency error for sidelink CA 698

6.4E.1.2 Frequency error for V2X concurrent operation 698

6.4E.1F Frequency error for Sidelink Unlicensed 698

6.4E.1F.1 Frequency error for SL-U concurrent operation 698

6.4E.2 Transmit modulation quality for V2X 698

6.4E.2.1 General 698

6.4E.2.2 Error Vector Magnitude for V2X 698

6.4E.2.2A Error Vector Magnitude for sidelink CA 698

6.4E.2.3 Carrier leakage for V2X 698

6.4E.2.3A Carrier leakage for sidelink CA 699

6.4E.2.4 In-band emissions for V2X 699

6.4E.2.4A In-band emissions for sidelink CA 699

6.4E.2.5 EVM equalizer spectrum flatness for V2X 699

6.4E.2.6 Transmit modulation quality for V2X concurrent operation 699

6.4E.2F Transmit modulation quality for Sidelink Unlicensed 699

6.4E.2F.0 General 699

6.4E.2F.1 Error Vector Magnitude 699

6.4E.2F.2 Carrier leakage 699

6.4E.2F.3 In-band emissions 700

6.4E.2F.4 EVM equalizer spectrum flatness 700

6.4E.2F.5 Transmit modulation quality for SL-U concurrent operation 700

6.4F Transmit signal quality for shared spectrum channel access 700

6.4F.1 Frequency error 700

6.4F.2 Transmit modulation quality 700

6.4F.2.0 General 700

6.4F.2.1 Error Vector Magnitude 700

6.4F.2.2 Carrier leakage 700

6.4F.2.3 In-band emissions 700

6.4F.2.4 EVM equalizer spectrum flatness 701

6.4F.2A Transmit modulation quality for CA 701

6.4F.2A.1 Transmit modulation quality for inter-band CA 701

6.4G Transmit signal quality for Tx Diversity 702

6.4G.1 Frequency error for Tx Diversity 702

6.4G.2 Transmit modulation quality for Tx Diversity 702

6.4G.2.0 General 702

6.4H Transmit signal quality for CA with UL MIMO 703

6.4H.1 Transmit signal quality for intra-band UL contiguous CA with UL MIMO 703

6.4H.1.1 Frequency error for intra-band UL contiguous CA with UL MIMO 703

6.4H.1.2 Transmit modulation quality for intra-band UL contiguous CA with UL MIMO 703

6.4H.1.2.0 General 703

6.4H.1.2.1 Error Vector Magnitude 703

6.4H.1.2.2 Carrier leakage 703

6.4H.1.2.3 In-band emissions 703

6.4H.1.3 Time alignment error for intra-band UL contiguous CA with UL MIMO 704

6.4H.1.4 Coherent UL MIMO requirement for intra-band UL contiguous CA with UL MIMO 704

6.4H.2 Void 704

6.4H.3 Transmit signal quality for inter-band UL CA with UL MIMO 704

6.4H.3.1 Frequency error for inter-band UL CA with UL MIMO 704

6.4H.3.2 Transmit modulation quality for inter-band UL CA with UL MIMO 704

6.4I (Reserved) 704

6.4J Transmit signal quality for ATG 704

6.4J.1 Frequency error for ATG 704

6.4J.2 Transmit modulation quality for ATG 704

6.4K (Reserved) 705

6.4L Transmit signal quality for CA with Tx Diversity 705

6.4L.1 Void 705

6.4L.2 Void 705

6.4L.3 Transmit signal quality for inter-band UL CA with Tx Diversity 705

6.4L.3.1 Frequency error for inter-band UL CA with Tx Diversity 705

6.4L.3.2 Transmit modulation quality for inter-band UL CA with Tx Diversity 705

6.5 Output RF spectrum emissions 705

6.5.1 Occupied bandwidth 705

6.5.2 Out of band emission 705

6.5.2.1 General 705

6.5.2.2 Spectrum emission mask 706

6.5.2.3 Additional spectrum emission mask 706

6.5.2.3.1 Requirements for network signalling value "NS\_35" 706

6.5.2.3.2 Requirements for network signalling value "NS\_04" 706

6.5.2.3.3 Requirements for network signalling values "NS\_03" and “NS\_03U” 707

6.5.2.3.4 Requirements for network signalling value "NS\_06" or “NS\_07” 708

6.5.2.3.5 Void 708

6.5.2.3.6 Void 708

6.5.2.3.7 Void 708

6.5.2.3.8 Requirements for network signalling value "NS\_27" 708

6.5.2.3.9 Requirements for network signalling value "NS\_21" 709

6.5.2.4 Adjacent channel leakage ratio 709

6.5.2.4.1 NR ACLR 710

6.5.2.4.2 UTRA ACLR 710

6.5.3 Spurious emissions 711

6.5.3.0 General 711

6.5.3.1 General spurious emissions 711

6.5.3.2 Spurious emissions for UE co-existence 711

6.5.3.3 Additional spurious emissions 719

6.5.3.3.1 Requirement for network signalling value "NS\_04" 720

6.5.3.3.2 Requirement for network signalling value "NS\_17" 720

6.5.3.3.3 Requirement for network signalling value "NS\_18" 720

6.5.3.3.4 Requirement for network signalling values "NS\_05" and “NS\_05U” 720

6.5.3.3.5 Requirement for network signalling values "NS\_43" and “NS\_43U” 721

6.5.3.3.6 Requirement for network signalling value "NS\_37" 721

6.5.3.3.7 Requirement for network signalling value "NS\_38" 721

6.5.3.3.8 Requirement for network signalling value "NS\_39" 721

6.5.3.3.9 Requirement for network signalling value "NS\_40" 722

6.5.3.3.10 Requirement for network signalling value "NS\_41" 722

6.5.3.3.11 Requirement for network signalling value "NS\_42" 722

6.5.3.3.12 Requirement for network signalling value "NS\_21" 723

6.5.3.3.13 Requirement for network signalling value "NS\_24" 723

6.5.3.3.14 Requirement for network signalling value "NS\_27" 723

6.5.3.3.15 Requirement for network signalling value "NS\_47" 723

6.5.3.3.16 Requirement for network signalling value "NS\_50" 724

6.5.3.3.17 Requirement for network signalling value "NS\_12" 724

6.5.3.3.18 Requirement for network signalling value "NS\_13" 724

6.5.3.3.19 Requirement for network signalling value "NS\_14" 725

6.5.3.3.20 Requirement for network signalling value "NS\_15" 725

6.5.3.3.21 Requirement for network signalling value "NS\_45" 725

6.5.3.3.22 Requirement for network signalling values "NS\_48" and "NS\_51" 726

6.5.3.3.23 Requirement for network signalling value "NS\_49" 726

6.5.3.3.24 Requirement for network signalling value "NS\_44" 726

6.5.3.3.25 Requirement for network signalling value "NS\_46" 727

6.5.3.3.26 Requirement for network signalling value "NS\_07" 727

6.5.3.3.27 Requirement for network signalling value “NS\_56” 727

6.5.3.3.28 Requirement for network signalling value “NS\_62” 728

6.5.4 Transmit intermodulation 728

6.5A Output RF spectrum emissions for CA 729

6.5A.0 General 729

6.5A.1 Occupied bandwidth for CA 729

6.5A.1.1 Void 729

6.5A.1.1a Occupied bandwidth for Intra-band contiguous CA 729

6.5A.1.2 Occupied bandwidth for Intra-band non-contiguous CA 729

6.5A.1.3 Occupied bandwidth for Inter-band CA 729

6.5A.2 Out of band emission for CA 729

6.5A.2.1 General 729

6.5A.2.2 Spectrum emission mask 730

6.5A.2.2.1 Spectrum emission mask for intra-band contiguous CA 730

6.5A.2.2.2 Spectrum emission mask for intra-band non-contiguous CA 730

6.5A.2.2.3 Spectrum emission mask for Inter-band CA 730

6.5.A.2.2.4 Void 731

6.5A.2.3 Additional spectrum emission mask for CA 731

6.5A.2.3.1 Additional spectrum emission mask for intra-band contiguous CA 731

6.5A.2.3.2 Additional spectrum emission mask for Intra-band non-contiguous CA 732

6.5A.2.3.3 Additional spectrum emission mask for Inter-band CA 732

6.5A.2.4 Adjacent channel leakage ratio 732

6.5A.2.4.1 NR ACLR 732

6.5A.2.4.2 UTRA ACLR 734

6.5A.3 Spurious emission for CA 734

6.5A.3.1 General spurious emissions 734

6.5A.3.2 Spurious emissions for UE co-existence 735

6.5A.3.2.0 General 735

6.5A.3.2.1 Spurious emissions for UE co-existence for intra-band contiguous CA 735

6.5A.3.2.2 Spurious emissions for UE co-existence for intra-band non-contiguous CA 737

6.5A.3.2.3 Spurious emissions for UE co-existence for Inter-band CA 738

6.5A.3.2.4 Void 744

6.5A.3.2.5 Void 744

6.5A.3.2.6 Void 744

6.5A.3.3 Additional spurious emissions for CA 744

6.5A.3.3.1 Additional spurious emissions for intra-band contiguous CA 744

6.5A.3.3.2 Additional spurious emissions for intra-band non-contiguous CA 745

6.5A.4 Transmit intermodulation for CA 746

6.5A.4.2.1 Transmit intermodulation for intra-band contiguous CA 746

6.5A.4.2.2 Void 746

6.5B Output RF spectrum emissions for NR-DC 746

6.5D Output RF spectrum emissions for UL MIMO 746

6.5D.1 Occupied bandwidth for UL MIMO 746

6.5D.2 Out of band emission for UL MIMO 747

6.5D.3 Spurious emission for UL MIMO 747

6.5D.4 Transmit intermodulation for UL MIMO 747

6.5E Output RF spectrum emissions for V2X 747

6.5E.1 Occupied bandwidth for V2X 747

6.5E.1.1 General 747

6.5E.1.1A Occupied bandwidth for sidelink CA 748

6.5E.1.2 Occupied bandwidth for V2X concurrent operation 748

6.5E.1F Occupied bandwidth for Sidelink Unlicensed 748

6.5E.1F.1 Occupied bandwidth for SL-U concurrent operation 748

6.5E.2 Out of band emission for V2X 748

6.5E.2.1 General 748

6.5E.2.2 Spectrum emission mask 748

6.5E.2.2.1 General 748

6.5E.2.2.1A Spectrum emission mask for sidelink CA 748

6.5E.2.2.2 Spectrum emission mask for V2X concurrent operation 749

6.5E.2.3 Additional Spectrum emission mask 749

6.5E.2.3.1 Requirements for network signalling value "NS\_33" 749

6.5E.2.3.2 Requirements for network signalling value "NS\_52" 749

6.5E.2.3.3 Requirements for network signalling value "NS\_06" 750

6.5E.2.4 Adjacent channel leakage ratio 750

6.5E.2.4.1 General 750

6.5E.2.4.1A ACLR for sidelink CA 750

6.5E.2.4.2 ACLR for V2X concurrent operation 750

6.5E.2F Out of band emission for Sidelink Unlicensed 750

6.5E.2F.1 General 750

6.5E.2F.2 Spectrum emission mask for operation with shared spectrum channel access 751

6.5E.2F.2.1 Spectrum emission mask for SL-U concurrent operation 751

6.5E.2F.3 Additional spectrum emission mask 751

6.5E.2F.4 Adjacent channel leakage ratio 751

6.5E.2F.4.1 Adjacent channel leakage ratio for SL-U concurrent operation 751

6.5E.3 Spurious emissions for V2X 751

6.5E.3.1 General spurious emissions 751

6.5E.3.1A Spurious emissions for sidelink CA 751

6.5E.3.2 Spurious emissions for UE co-existence 751

6.5E.3.2A Spurious emissions band UE co-existence for sidelink CA 752

6.5E.3.3 Spurious emissions for UE co-existence for V2X concurrent operation 752

6.5E.3.4 Additional spurious emissions requirements for V2X 753

6.5E.3.4.1 General 753

6.5E.3.4.2 Requirements for network signalling value "NS\_33" 753

6.5E.3.4.3 Void 753

6.5E.3F Spurious emissions for Sidelink Unlicensed 753

6.5E.3F.0 General 753

6.5E.3F.1 General spurious emissions 754

6.5E.3F.2 Spurious emissions for UE co-existence 754

6.5E.3F.2.1 Spurious emissions for UE co-existence for SL-U concurrent operation 754

6.5E.3F.3 Additional spurious emissions 754

6.5E.3F.3.0 General 754

6.5E.4 Transmit intermodulation 754

6.5E.4.1 General 754

6.5E.4.1A Transmit intermodulation for sidelink CA 754

6.5E.4.2 Transmit intermodulation for V2X concurrent operation 754

6.5F Output RF spectrum emissions for shared spectrum channel access 755

6.5F.1 Occupied bandwidth 755

6.5F.2 Out of band emission 755

6.5F.2.1 General 755

6.5F.2.2 Spectrum emission mask for operation with shared spectrum channel access 755

6.5F.2.2.0 General 755

6.5F.2.2.1 Spectrum emission mask for non-transmitted channels 756

6.5F.2.3 Additional spectrum emission mask 756

6.5F.2.4 Adjacent channel leakage ratio 756

6.5F.2.4.0 General 756

6.5F.2.4.1 Shared spectrum channel access ACLR 756

6.5F.2.4.2 Additional requirement for network signalled value "NS\_29" 756

6.5F.2A Out of band emission for CA 757

6.5F.2A.1 Spectrum emission mask for CA 757

6.5F.2A.1.1 Spectrum emission mask for Inter-band CA 757

6.5F.2A.1.2 Spectrum emission mask for Intra-band contiguous CA 757

6.5F.2A.1.2.1 General 757

6.5F.2A.1.2.2 Intra-band contiguous CA spectrum emission mask for non-transmitted channels 758

6.5F.2A.2 Adjacent channel leakage ratio for CA 758

6.5F.2A.2.1 Adjacent channel leakage ratio for inter-band CA 758

6.5F.2A.2.2 Adjacent channel leakage ratio for intra-band contiguous CA 758

6.5F.3 Spurious emissions 758

6.5F.3.0 General 758

6.5F.3.1 General spurious emissions 759

6.5F.3.2 Spurious emissions for UE co-existence 759

6.5F.3.3 Additional spurious emissions 759

6.5F.3.3.0 General 759

6.5F.3.3.1 Requirement for network signalling value "NS\_28" 759

6.5F.3.3.2 Requirement for network signalling value "NS\_29" 759

6.5F.3.3.3 Requirement for network signalling value "NS\_30" 761

6.5F.3.3.4 Requirement for network signalling value "NS\_31" 762

6.5F.3.3.5 Requirements for network signalling value "NS\_53" or "NS\_54" or "NS\_60" or "NS\_66" or "NS\_67" or "NS\_71" 763

6.5F.3.3.6 Requirements for network signalling value "NS\_58" 763

6.5F.3.3.7 Requirements for network signalling value "NS\_61" 763

6.5F.3.3.8 Requirements for network signalling value “NS\_63” or “NS\_69” 763

6.5F.3.3.9 Requirements for network signalling value “NS\_64” 764

6.5F.3A Spurious emissions for CA 764

6.5F.3A.0 General 764

6.5F.3A.1 General spurious emissions 765

6.5F.3A.2 Spurious emissions for UE co-existence 765

6.5F.3A.3 Additional spurious emissions 765

6.5F.3A.3.0 General 765

6.5F.3A.3.1 Requirements for network signalling value "CA\_NS\_53" or "CA\_NS\_54" 765

6.5F.4 Transmit intermodulation 765

6.5G Output RF spectrum emissions for Tx Diversity 765

6.5G.1 Occupied bandwidth for Tx Diversity 765

6.5G.2 Out of band emission for Tx Diversity 766

6.5G.3 Spurious emission for Tx Diversity 766

6.5G.4 Transmit intermodulation for Tx Diversity 766

6.5H Output RF spectrum emissions for CA with UL MIMO 766

6.5H.1 Output RF spectrum emissions for intra-band UL contiguous CA with UL MIMO 766

6.5H.1.1 Occupied bandwidth for intra-band UL contiguous CA with UL MIMO 766

6.5H.1.2 Out of band emission for intra-band UL contiguous CA with UL MIMO 766

6.5H.1.3 Spurious emission for intra-band UL contiguous CA with UL MIMO 766

6.5H.1.4 Transmit intermodulation for intra-band UL contiguous CA with UL MIMO 767

6.5H.2 Void 767

6.5H.3 Output RF spectrum emissions for inter-band UL CA with UL MIMO 767

6.5H.3.1 Occupied bandwidth for inter-band UL CA with UL MIMO 767

6.5H.3.2 Out of band emission for inter-band UL CA with UL MIMO 767

6.5H.3.3 Spurious emission for inter-band UL CA with UL MIMO 767

6.5H.3.4 Transmit intermodulation for inter-band UL CA with UL MIMO 767

6.5I (Reserved) 767

6.5J Output RF spectrum emissions for ATG 768

6.5J.1 Occupied bandwidth for ATG 768

6.5J.2 Out of band emission for ATG 768

6.5J.2.1 General 768

6.5J.2.2 Spectrum emission mask 768

6.5J.2.3 Adjacent channel leakage ratio 768

6.5J.3 Spurious emissions for ATG 768

6.5K Output RF spectrum emissions for Aerial UE 769

6.5K.1 Occupied bandwidth for Aerial UE 769

6.5K.2 Out of band emission for Aerial UE 769

6.5K.3 Spurious emissions for Aerial UE 769

6.5K.3.0 General 769

6.5K.3.1 General spurious emissions 769

6.5K.3.2 Spurious emissions for UE co-existence 769

6.5K.3.3 Additional spurious emissions 769

6.5K.3.3.1 Requirement for network signalling value "NS\_UAV\_44" 769

6.5K.3.3.2 Requirement for network signalling value "NS\_UAV\_46" 769

6.5K.3.3.3 Requirement for network signalling value “NS\_UAV\_70" 770

6.5L Output RF spectrum emissions for CA with Tx Diversity 770

6.5L.1 Void 770

6.5L.2 Void 770

6.5L.3 Output RF spectrum emissions for inter-band UL CA with Tx Diversity 770

6.5L.3.1 Occupied bandwidth for inter-band UL CA with Tx Diversity 770

6.5L.3.2 Out of band emission for inter-band UL CA with Tx Diversity 770

6.5L.3.3 Spurious emission for inter-band UL CA with Tx Diversity 770

6.5L.3.4 Transmit intermodulation for inter-band UL CA with Tx Diversity 770

6.6 Void 770

6.6E Time alignment error 771

7 Receiver characteristics 772

7.1 General 772

7.1A General 773

7.1F General 773

7.1G (Reserved) 773

7.1H (Reserved) 773

7.1I General 773

7.1J General for ATG 773

7.1K (Reserved) 773

7.1L (Reserved) 773

7.2 Diversity characteristics 773

7.2J Diversity characteristics for ATG 774

7.3 Reference sensitivity 774

7.3.1 General 774

7.3.2 Reference sensitivity power level 774

7.3.3 ΔRIB,c 784

7.3A Reference sensitivity for CA 784

7.3A.1 General 784

7.3A.2 Reference sensitivity power level for CA 785

7.3A.2.1 Reference sensitivity power level for Intra-band contiguous CA 785

7.3A.2.2 Reference sensitivity power level for Intra-band non-contiguous CA 786

7.3A.2.3 Reference sensitivity power level for Inter-band CA 788

7.3A.2.4 Void 788

7.3A.3 ΔRIB,c for CA 789

7.3A.3.1 General 789

7.3A.3.2 ΔRIB,c for Inter-band CA 789

7.3A.3.2.1 ΔRIB,c for two bands 789

7.3A.3.2.2 Void 791

7.3A.3.2.3 ΔRIB,c for three bands 792

7.3A.3.2.4 ΔRIB,c for four bands 796

7.3A.3.2.5 ΔRIB,c for five bands 799

7.3A.3.2.6 ΔRIB,c for six bands 800

7.3A.3.3 ΔRIB,c for Intra-band CA 800

7.3A.4 Reference sensitivity exceptions due to harmonic interference for CA 800

7.3A.5 Reference sensitivity exceptions due to intermodulation interference due to 2UL CA 813

7.3A.6 Reference sensitivity exceptions due to cross band isolation for CA 859

7.3A.7 Lower-MSD requirements for inter-band CA 864

7.3B Reference sensitivity for NR-DC 865

7.3C Reference sensitivity for SUL 865

7.3C.1 General 865

7.3C.2 Reference sensitivity power level for SUL 865

7.3C.3 ΔRIB,c for SUL 868

7.3C.3.1 General 868

7.3C.3.2 SUL band combination 869

7.3C.3.2.1 ΔRIB,c for two bands 869

7.3C.3.2.2 ΔRIB,c for three bands 869

7.3C.3.2.3 ΔRIB,c for four bands 870

7.3D Reference sensitivity for UL MIMO 870

7.3E Reference sensitivity for V2X 870

7.3E.1 General 870

7.3E.2 Minimum requirements 871

7.3E.2A Minimum requirements for Sidelink CA 871

7.3E.2A.1 Reference sensitivity power level for Sidelink CA 871

7.3E.2F Minimum requirements for Sidelink Unlicensed 872

7.3E.2F.1 General 872

7.3E.2F.2 Reference sensitivity power level 872

7.3E.3 Reference sensitivity power level for V2X concurrent operation 873

7.3E.3.1 General 873

7.3E.3F Minimum requirements for SL-U concurrent operation 874

7.3E.3F.1 Reference sensitivity power level for SL-U concurrent operation 874

7.3F Reference sensitivity for shared spectrum channel access 874

7.3F.1 General 874

7.3F.2 Reference sensitivity power level 874

7.3F.3 Void 875

7.3F.4 Void 875

7.3F.4A Shared spectrum channel access CA 875

7.3F.4A.1 Intra-band contiguous shared spectrum channel access CA 875

7.3F.5 Void 875

7.3F.5.1 Void 875

7.3F.5.2 Void 875

7.3F.5.3 Void 875

7.3G Reference sensitivity for Tx Diversity 875

7.3G.5 Void 876

7.3G.5.0 Void 876

7.3H (Reserved) 876

7.3I Reference sensitivity for (e)RedCap 876

7.3I.1 General 876

7.3I.2 Reference sensitivity power level for RedCap 876

7.3I.3 Reference sensitivity power level for eRedCap 880

7.3J Reference sensitivity for ATG 880

7.3J.1 General 880

7.3J.2 Reference sensitivity power level 881

7.3K (Reserved) 881

7.3L (Reserved) 881

7.4 Maximum input level 881

7.4A Maximum input level for CA 881

7.4A.1 Maximum input level for Intra-band contiguous CA 881

7.4A.2 Maximum input level for Intra-band non-contiguous CA 882

7.4A.3 Maximum input level for Inter-band CA 882

7.4B Maximum input level for NR-DC 882

7.4D Maximum input level for UL MIMO 882

7.4E Maximum input level for V2X 883

7.4E.1 General 883

7.4E.1A Maximum input level for Sidelink CA 883

7.4E.1F General requirement for Sidelink Unlicensed 883

7.4E.2 Maximum input level for V2X concurrent operation 883

7.4E.2F Maximum input level for SL-U concurrent operation 884

7.4F (Reserved) 884

7.4G (Reserved) 884

7.4H (Reserved) 884

7.4I (Reserved) 884

7.4J Maximum input level for ATG 884

7.4K (Reserved) 884

7.4L (Reserved) 884

7.5 Adjacent channel selectivity 884

7.5A Adjacent channel selectivity for CA 887

7.5A.1 Adjacent channel selectivity for Intra-band contiguous CA 887

7.5A.2 Adjacent channel selectivity Intra-band non-contiguous CA 889

7.5A.3 Adjacent channel selectivity Inter-band CA 889

7.5B Adjacent channel selectivity for NR-DC 889

7.5D Adjacent channel selectivity for UL MIMO 889

7.5E Adjacent channel selectivity for V2X 890

7.5E.1 General 890

7.5E.1A Adjacent channel selectivity requirement for Sidelink CA 891

7.5E.1F General requirement for Sidelink Unlicensed 892

7.5E.2 Adjacent channel selectivity for V2X concurrent operation 892

7.5E.2F Adjacent channel selectivity for SL-U concurrent operation 892

7.5F Adjacent channel selectivity for shared spectrum channel access 892

7.5F.1 General 892

7.5F.1A Adjacent channel selectivity for shared spectrum channel access CA 893

7.5F.1A.1 Intra-band contiguous shared spectrum channel access CA 893

7.5F.2 Void 894

7.5G (Reserved) 894

7.5H (Reserved) 894

7.5I (Reserved) 894

7.5J Adjacent channel selectivity for ATG 894

7.5K (Reserved) 896

7.5L (Reserved) 896

7.6 Blocking characteristics 896

7.6.1 General 896

7.6.2 In-band blocking 896

7.6.3 Out-of-band blocking 899

7.6.4 Narrow band blocking 902

7.6A Blocking characteristics for CA 904

7.6A.1 General 904

7.6A.2 In-band blocking for CA 904

7.6A.2.1 In-band blocking for Intra-band contiguous CA 904

7.6A.2.2 In-band blocking for Intra-band non-contiguous CA 905

7.6A.2.3 In-band blocking for Inter-band CA 905

7.6A.3 Out-of-band blocking for CA 906

7.6A.3.1 Out-of-band blocking for Intra-band contiguous CA 906

7.6A.3.2 Out-of-band blocking for Intra-band non-contiguous CA 907

7.6A.3.3 Out-of-band blocking for Inter-band CA 907

7.6A.4 Narrow band blocking for CA 909

7.6A.4.1 Narrow band blocking for Intra-band contiguous CA 909

7.6A.4.2 Narrow band blocking for Intra-band non-contiguous CA 909

7.6A.4.3 Narrow band blocking for Inter-band CA 910

7.6B Blocking characteristics for NR-DC 910

7.6C Blocking characteristics for SUL 910

7.6C.1 General 910

7.6C.2 In-band blocking for SUL 910

7.6C.3 Out-of-band blocking for SUL 910

7.6C.4 Narrow band blocking for SUL 911

7.6D Blocking characteristics for UL MIMO 911

7.6E Blocking characteristics for V2X 911

7.6E.1 General 911

7.6E.2 In-band blocking 911

7.6E.2.1 General 911

7.6E.2.1A In-band blocking for Sidelink CA 912

7.6E.2.2 In-band blocking for V2X concurrent operation 913

7.6E.2.2F In-band blocking for SL-U concurrent operation 913

7.6E.3 Out-of-band blocking 913

7.6E.3.1 General 913

7.6E.3.1A Out-of-band blocking for Sidelink CA 914

7.6E.3.2 Out-of-band blocking for V2X concurrent operation 915

7.6E.3.2F Out-of-band blocking for SL-U concurrent operation 915

7.6E.3F Out-of-band blocking for Sidelink Unlicensed 915

7.6F Blocking characteristics for shared spectrum channel access 915

7.6F.1 General 915

7.6F.2 In-band blocking 915

7.6F.2.1 General 915

7.6F.2.2 Void 916

7.6F.2A In-band blocking for shared spectrum CA 916

7.6F.2A.1 Intra-band contiguous shared spectrum channel access CA 916

7.6F.3 Out-of-band blocking 917

7.6F.3.1 General 917

7.6F.3.2 Void 918

7.6F.3A Out-of-band blocking for shared spectrum CA 918

7.6F.3A.1 Intra-band contiguous shared spectrum channel access CA 918

7.6G (Reserved) 918

7.6H (Reserved) 918

7.6I (Reserved) 918

7.6J Blocking characteristics for ATG 919

7.6J.1 General 919

7.6J.2 In-band blocking for ATG 919

7.6J.3 Out-of-band blocking for ATG 919

7.6K (Reserved) 919

7.6L (Reserved) 919

7.7 Spurious response 919

7.7A Spurious response for CA 920

7.7A.1 Spurious response for Intra-band contiguous CA 920

7.7A.2 Spurious response for Intra-band non-contiguous CA 920

7.7A.3 Spurious response for Inter-band CA 921

7.7B Spurious response for NR-DC 921

7.7D Spurious response for UL MIMO 921

7.7E Spurious response for V2X 921

7.7E.1 General 921

7.7E.1A Spurious response requirements for Sidelink CA 922

7.7E.1F General requirement for Sidelink Unlicensed 922

7.7E.2 Spurious response for V2X concurrent operation 922

7.7E.2F Spurious response for SL-U concurrent operation 922

7.7F Spurious response for shared spectrum channel access 922

7.7F.1 General 922

7.7F.1A Spurious response for shared spectrum channel access CA 923

7.7F.1A.1 Intra-band contiguous shared spectrum channel access CA 923

7.7F.2 Void 923

7.7G (Reserved) 923

7.7H (Reserved) 923

7.7I (Reserved) 923

7.7J Spurious response for ATG 924

7.7K (Reserved) 924

7.7L (Reserved) 924

7.8 Intermodulation characteristics 924

7.8.1 General 924

7.8.2 Wide band Intermodulation 924

7.8A Intermodulation characteristics for CA 926

7.8A.1 General 926

7.8A.2 Wide band intermodulation for CA 926

7.8A.2.1 Wide band intermodulation for Intra-band contiguous CA 926

7.8A.2.2 Wide band intermodulation for Intra-band non-contiguous CA 927

7.8A.2.3 Wide band intermodulation for Inter-band CA 927

7.8B Intermodulation characteristics for NR-DC 928

7.8D Intermodulation characteristics for UL MIMO 928

7.8E Intermodulation characteristics for V2X 928

7.8E.1 General 928

7.8E.2 Wide band Intermodulation 928

7.8E.2.1 General 928

7.8E.2.2 Wide band Intermodulation for V2X concurrent operation 929

7.8E.2.2A Wide band intermodulation for Sidelink CA 929

7.8E.2.2F Wide band Intermodulation for SL-U concurrent operation 929

7.8E.2F Wide band Intermodulation for Sidelink Unlicensed 930

7.8F Intermodulation characteristics for shared spectrum channel access 930

7.8F.1 General 930

7.8F.2 Wide band Intermodulation 930

7.8G (Reserved) 930

7.8H (Reserved) 930

7.8I (Reserved) 931

7.8J Intermodulation characteristics for ATG 931

7.8J.1 General 931

7.8J.2 Wide band intermodulation for ATG 931

7.8K (Reserved) 931

7.8L (Reserved) 931

7.9 Spurious emissions 931

7.9A Spurious emissions for CA 931

7.9A.1 Void 931

7.9A.2 Void 931

7.9A.3 Spurious emissions for Inter-band CA 931

7.9B Spurious emissions for NR-DC 932

7.9J Spurious emissions for ATG 932

7.10 Power imbalance 932

7.10A Power imbalance for CA 932

7.10A.1 General 932

7.10A.2 Minimum requirement 932

Annex A (normative): Measurement channels 934

A.1 General 934

A.2 UL reference measurement channels 934

A.2.1 General 934

A.2.2 Reference measurement channels 936

A.2.2.1 DFT-s-OFDM Pi/2-BPSK 936

A.2.2.2 DFT-s-OFDM QPSK 938

A.2.2.3 DFT-s-OFDM 16QAM 939

A.2.2.4 DFT-s-OFDM 64QAM 940

A.2.2.5 DFT-s-OFDM 256QAM 942

A.2.2.6 CP-OFDM QPSK 943

A.2.2.7 CP-OFDM 16QAM 945

A.2.2.8 CP-OFDM 64QAM 947

A.2.2.9 CP-OFDM 256QAM 949

A.2.3 Reference measurement channels for TDD 952

A.2.3.1 DFT-s-OFDM Pi/2-BPSK 952

A.2.3.2 DFT-s-OFDM QPSK 952

A.2.3.3 DFT-s-OFDM 16QAM 952

A.2.3.4 DFT-s-OFDM 64QAM 952

A.2.3.5 DFT-s-OFDM 256QAM 953

A.2.3.6 CP-OFDM QPSK 953

A.2.3.7 CP-OFDM 16QAM 953

A.2.3.8 CP-OFDM 64QAM 953

A.2.3.9 CP-OFDM 256QAM 954

A.3 DL reference measurement channels 954

A.3.1 General 954

A.3.2 DL reference measurement channels for FDD 957

A.3.2.1 General 957

A.3.2.2 FRC for receiver requirements for QPSK 958

A.3.2.3 FRC for maximum input level for 64QAM 961

A.3.2.4 FRC for maximum input level for 256 QAM 964

A.3.2.5 FRC for maximum input level for 1024 QAM 967

A.3.3 DL reference measurement channels for TDD 970

A.3.3.1 General 970

A.3.3.2 FRC for receiver requirements for QPSK 971

A.3.3.3 FRC for maximum input level for 64QAM 974

A.3.3.4 FRC for maximum input level for 256 QAM 977

A.3.3.5 FRC for maximum input level for 1024 QAM 980

A.4 CSI reference measurement channels 983

A.5 OFDMA Channel Noise Generator (OCNG) 983

A.5.1 OCNG Patterns for FDD 983

A.5.1.1 OCNG FDD pattern 1: Generic OCNG FDD Pattern for all unused REs 983

A.5.2 OCNG Patterns for TDD 983

A.5.2.1 OCNG TDD pattern 1: Generic OCNG TDD Pattern for all unused REs 983

A.6 Void 984

A.7 V2X reference measurement channels 984

A.7.1 General 984

A.7.2 FRC for V2X receiver requirements for QPSK 984

A.7.3 FRC for maximum input level for 64QAM 986

A.7.4 FRC for maximum input level for 256QAM 987

Annex B (informative): Void 990

Annex C (informative): Downlink physical channels 991

C.1 General 991

C.2 Setup 991

C.3 Connection 991

C.3.1 Measurement of Receiver Characteristics 991

Annex D (normative): Characteristics of the interfering signal 992

D.1 General 992

D.2 Interference signals 992

Annex E (normative): Environmental conditions 994

E.1 General 994

E.2 Environmental 994

E.2.1 Temperature 994

E.2.2 Voltage 994

E.2.3 Vibration 995

Annex F (normative): Transmit modulation 996

F.0 General 996

F.1 Measurement Point 996

F.2 Basic Error Vector Magnitude measurement 996

F.3 Basic in-band emissions measurement 997

F.4 Modified signal under test 998

F.5 Window length 1000

F.5.1 Timing offset 1000

F.5.2 Window length 1000

F.5.3 Window length for normal CP 1000

F.5.4 Window length for Extended CP 1001

F.5.5 Window length for PRACH 1002

F.6 Averaged EVM 1003

F.7 Spectrum Flatness 1004

F.8 EVM measurement for multiple Tx 1004

F.9 Phase offset measurement for DMRS bundling 1004

F.9.1 Measurement point 1004

F.9.2 Symbols used 1004

F.9.3 Modified test signal 1004

F.9.4 Phase offset measurement 1005

F.10 EVM for UL MIMO 1005

F10.1 General 1005

F10.2 MIMO Equalization 1006

F10.3 Layer processing 1007

Annex G (normative): Difference of relative phase and power errors 1008

G.0 General 1008

G.1 Measurement Point 1008

G.2 Relative Phase Error Measurement 1008

G.2.1 Symbols and subcarriers used 1008

G.2.2 CFO (carrier frequency offset) correction 1009

G.2.3 Steps of the measurement method 1009

Annex H (informative): Void 1010

Annex I (informative): Void 1011

Annex J (informative): Void 1012

Annex K (informative): Void 1013

Annex L (normative): ModifiedMPR-Behavior 1014

L.1 Indication of modified MPR behavior 1014

Annex M (normative): Declared Supported Post Antenna Gain for UE 1017

M.1 FRMCS operating bands 1017

Annex N (informative): Change history 1018